SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( bdz_44114
	Type ( Engine )
	WagonShape ( bdz_44114.s )
	
	Comment ( Eng created by ZSR - http://csd.webzdarma.cz )
	Comment ( Datum: 19/12/2008 )
	Comment ( Version: 1.03 )Comment ( Svetla: 2 reflektory halogen )

	

comment	( Overall physics )

	Size ( 3.12m 4.67m 15.97m )
	CentreOfGravity ( 0m 2.25m 0m )
	Mass ( 84t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3.12m 4.67m 15.97m ) )


comment	( Coupling )

comment ( Rear Coupler )

	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 5e6N/m 0 )
			Damping ( 1e6N/m/s 0 )
			Break ( 2e7N 0 )
			r0 ( 15cm 1e9 )
		)
		CouplingHasRigidConnection ()
		Velocity ( 0.1m/s )
	)
	

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	


comment	( Adhesion and Friction )

	Adheasion ( 0.07 0.75 1.3 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*85t )
	DerailBufferForce ( 800kN )
	NumWheels (	4 )
	Friction (
		3000N/m/s		0		11.5mph		25N/m/s		2.2
		5.1N/rad/s		1		-1rad/s		0		1
	)



comment	( Wagon Brakes )

 	Comment ( P=52kN, G=32kN )
 	
	MaxBrakeForce( 52kN )
	MaxHandbrakeForce( 18kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 2.5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )
	
comment	( Freight, IntakePoint )
	
		

comment	( Lights )


 
comment ( svetelne kuzely ) 

	Lights ( 36
		Light (
  comment ( Svetelny kuzel dalkovy )
  Type ( 1 )
  Conditions (
  Headlight ( 3 )
  Unit ( 2 )
  Control ( 2 )
  )
  FadeIn ( 1 )
  FadeOut ( 1 )
  Cycle ( 0 )
  States ( 1
  State (
  Duration ( 0 )
  LightColour ( FFFFEBA4 )
  Position ( 0.0 3 3 )
  Angle ( 10 )
  Transition ( 1 )
  Radius ( 300 )
  )
  )
  )
  Light (
  comment ( Svetelny kuzel tlumeny )
  Type ( 1 )
  Conditions (
  Headlight ( 2 )
  Unit ( 2 )
  Control ( 2 )
  )
  FadeIn ( 0.5 )
  FadeOut ( 0.5 )
  States ( 1
  State (
  Duration ( 0 )
  LightColour ( FF444444 )
  Position ( 0.0 3 3 )
  Angle ( 30 )
  Transition ( 1 )
  Radius ( 150 )
				)
			)
		)

comment ( Definice svetel pro predni stanoviste v cele vlaku )



		Light (
			comment ( reflektor dalkovy pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( 0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)		
		Light (
			comment ( reflektor dalkovy levy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( -0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny levy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)		
		

		
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.845 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.84 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.845 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.84 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)		
		Light (
			comment ( Zadni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.845 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.84 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		
comment ( Definice svetel pro predni stanoviste na postrku )

		Light (
			comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.56 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.56 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)


comment ( Definice svetel pro zadni stanoviste v cele vlaku )

		Light (
			comment ( reflektor dalkovy pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( 0.1 3.65 -7.33 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor dalkovy levy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBA4 )
					Position ( -0.1 3.65 -7.33 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)

		Light (
			comment ( reflektor tlumeny pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.1 3.65 -7.33 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny levy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.1 3.65 -7.33 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)


		
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.845 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.84 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
comment ( Definice svetel pro zadni stanoviste na postrku )
		
		Light (
			comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.56 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light ( 
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.56 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)



		
comment ( Definice svetel pro loko ovladanou PC v normanim smeru )


		Light (
			comment ( PC reflektor pravy predni tlumeny v noci )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor levy predni tlumeny v noci )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)		
		
		Light (
			comment ( PC reflektor pravy predni tlumeny ve dne za deste )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor levy predni tlumeny ve dne za deste )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)

		
		Light (
			comment ( PC reflektor pravy predni tlumeny ve dne za snehu )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( 0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor levy predni tlumeny ve dne za snehu )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Coupling ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 1 )
				Weather ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFEBA4 )
					Position ( -0.1 3.65 7.33 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)

	
		
		Light (
			comment ( PC predni leve v cele soupravy normalni smer )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( FFFFE085 )
					Position ( -0.84 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		Light (
			comment ( PC predni prave v cele soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.845 1.87 7.425 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC koncove leve na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.56 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC koncove prave na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.56 1.87 -7.425 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		

comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Leve predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.84 1.87 7.425 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Prave predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position (0.845 1.87 7.425 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( -0.84 1.87 -7.425 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Prave zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80F0E3B5 )
					Position ( 0.845 1.87 -7.425 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
			)
		)
	)

comment	( EngSound )

	Sound ( "242eng.sms" )


)

Engine ( bdz_44114   

comment	( Description )

	Wagon ( bdz_44114 )

	
comment	( Basic physical engine data )

	Type ( Electric )
	MaxPower ( 3140kW )
	MaxForce ( 700kN )	
	MaxContinuousForce ( 688kN )
	MaxCurrent ( 2450A ) 
	MaxVelocity ( 130kmh )
	DieselEngineSpeedOfMaxTractiveEffort( 0mph )  
	WheelRadius ( 0.625m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 1e9mph )
	NumWheels ( 4 )

	
comment	( CabSound and Views )

	Sound ( "242cab.sms" )
	
	CabView ( "cd242.cvf" )
	HeadOut ( 1.7m 3.2m 5.9m )
	


comment	( Brakes )


	AirBrakesAirCompressorPowerRating( 1.9 )
	AirBrakesMainMinResAirPressure( 56 )
	AirBrakesMainMaxAirPressure( 130 )
	AirBrakesMainResVolume( 39 )
	AirBrakesAirCompressorWattage( 34kW )
	AirBrakesCompressorRestartPressure( 105 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
	AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 0 )

	EngineBrakesControllerMinPressureReduction( 2.35 ) 
	TrainBrakesControllerMinPressureReduction( 2.35 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 1.5 )
	TrainBrakesControllerMaxApplicationRate( 2.8 )
	EngineBrakesControllerMaxReleaseRate( 1.5 )
	TrainBrakesControllerMaxReleaseRate( 2.8 ) 
	EngineBrakesControllerMaxQuickReleaseRate( 15 )
	TrainBrakesControllerMaxQuickReleaseRate( 15 )
	EngineBrakesControllerEmergencyApplicationRate( 30 )
	TrainBrakesControllerEmergencyApplicationRate( 24 ) 
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 ) 
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 23.2 ) comment ( 5bar-3.4bar=1.6bar=23.2psi [4/284] )
	TrainBrakesControllerFullServicePressureDrop( 23.2 )

	DynamicBrakesMinUsableSpeed( 9 )
	DynamicBrakesMaximumEffectiveSpeed( 80 )
	DynamicBrakesMaximumForce( 100kN )
	DynamicBrakesResistorCurrentLimit ( 750 )
	DynamicBrakesCutInSpeed( 3 )
	DynamicBrakesMaxAirBrakePressure ( 100 )
	DynamicBrakesFadingSpeed( 10 )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 90 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 7 )


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Dynamic" )

	EngineBrakesControllerDirectControlExponent( 1 )

	DoesBrakeCutPower ( 0 )

comment ( Monitors )


EmergencyStopMonitor(
   		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)

	AWSMonitor(
		MonitoringDeviceMonitorTimeLimit( -1 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)
	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 20 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		)
		
	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 154 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		)

	 
Comment	( Controllers )

        EngineControllers (
	Throttle ( 0 1 0.03 0 
                NumNotches ( 63 
				Notch ( 0		0 Dummy )
				Notch ( 0.03	0 Dummy )
				Notch ( 0.031	0 Dummy )
				Notch ( 0.06	0 Dummy )
				Notch ( 0.061	0 Dummy )
				Notch ( 0.09	0 Dummy )
				Notch ( 0.091	0 Dummy )
				Notch ( 0.12	0 Dummy )
				Notch ( 0.121	0 Dummy )
				Notch ( 0.15	0 Dummy )
				Notch ( 0.151	0 Dummy )
				Notch ( 0.18	0 Dummy )
				Notch ( 0.181	0 Dummy )
				Notch ( 0.21	0 Dummy )
				Notch ( 0.211	0 Dummy )
				Notch ( 0.24	0 Dummy )
				Notch ( 0.241	0 Dummy )
				Notch ( 0.27	0 Dummy )
				Notch ( 0.271	0 Dummy )
				Notch ( 0.3 	0 Dummy )
				Notch ( 0.301 	0 Dummy )
				Notch ( 0.33	0 Dummy )
				Notch ( 0.331	0 Dummy )
				Notch ( 0.36	0 Dummy )
				Notch ( 0.361	0 Dummy )
				Notch ( 0.39	0 Dummy )
				Notch ( 0.391	0 Dummy )
				Notch ( 0.42	0 Dummy )
				Notch ( 0.421	0 Dummy )
				Notch ( 0.45	0 Dummy )
				Notch ( 0.451	0 Dummy )
				Notch ( 0.48	0 Dummy )
				Notch ( 0.481	0 Dummy )
				Notch ( 0.51	0 Dummy )
				Notch ( 0.511	0 Dummy )
				Notch ( 0.54	0 Dummy )
				Notch ( 0.541	0 Dummy )
				Notch ( 0.57	0 Dummy )
				Notch ( 0.571	0 Dummy )
				Notch ( 0.6 	0 Dummy )
				Notch ( 0.601 	0 Dummy )
				Notch ( 0.63	0 Dummy )
				Notch ( 0.631	0 Dummy )
				Notch ( 0.66	0 Dummy )
				Notch ( 0.661	0 Dummy )
				Notch ( 0.69	0 Dummy )
				Notch ( 0.691	0 Dummy )
				Notch ( 0.72	0 Dummy )
				Notch ( 0.721	0 Dummy )
				Notch ( 0.75	0 Dummy )
				Notch ( 0.751	0 Dummy )
				Notch ( 0.78	0 Dummy )
				Notch ( 0.781	0 Dummy )
				Notch ( 0.81	0 Dummy )
				Notch ( 0.811	0 Dummy )
				Notch ( 0.84	0 Dummy )
				Notch ( 0.841	0 Dummy )
				Notch ( 0.87	0 Dummy )
				Notch ( 0.871	0 Dummy )
				Notch ( 0.9 	0 Dummy )
				Notch ( 0.93	0 Dummy )
				Notch ( 0.96	0 Dummy )
				Notch ( 1		0 Dummy )
				)
			)

	 Brake_Engine ( 0 1 0.20 1
                NumNotches ( 1
                    Notch ( 0       1 Dummy )                    
                )
        ) 

            Brake_Train ( 0 1 0.075 0
                  NumNotches ( 6
                    Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.1  0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.2  0 TrainBrakesControllerNeutralhandleOffStart )		 
                    Notch ( 0.3  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
		        Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
	Brake_Dynamic ( 0 1 0.07 0 
                NumNotches ( 16
                    Notch ( 0     0 Dummy )
                    Notch ( 0.07  0 Dummy )
                    Notch ( 0.14  0 Dummy )
                    Notch ( 0.21  0 Dummy )
                    Notch ( 0.28  0 Dummy )
                    Notch ( 0.35  0 Dummy )
		    Notch ( 0.42  0 Dummy )
                    Notch ( 0.49  0 Dummy )
                    Notch ( 0.56  0 Dummy )
                    Notch ( 0.63  0 Dummy )
                    Notch ( 0.70  0 Dummy )
		    Notch ( 0.77  0 Dummy )
                    Notch ( 0.84  0 Dummy )
                    Notch ( 0.91  0 Dummy )
                    Notch ( 0.98  0 Dummy )
		    Notch ( 1.00  0 Dummy )
                )
            )     

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
	    
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
 		PantographToggle1 ( 0 1 0 )
		PantographToggle2 ( 0 1 0 )
		PantographToggle_4 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	
Comment	( Operations )


	 Name ( "BDZ 44 114.7" )
	 Description (
	  "Rada 242 CD je univerzální elektrická skrínová lokomotiva, pouzívaná v nákladní i osobní doprave.\n\n"+
	  "Typ Bo'-Bo', napeti 25 kV 50Hz.\n\n"+
	  "Délka pres nárazniky: 16,44 m\n\n"+
	  "Prumer hnacích kol: 1250 mm\n\n"+
	  "Hmotnost ve sluzbe: 84 t\n\n"+
	  "Trvaly vykon trakcních motoru: 3080 kW\n\n"+
	  "Max. rychlost 120 km/h\n\n"+
	  "Ovladani a proudy v MSTS:\n\n"+
	  "Maximalni proud (nadproudova ochrana): 1250A\n\n"+
	  "Trvaly proud: 1100A\n\n"+
	  "Hodinovy proud: 1140A\n\n"+
	  "15 minutovy proud: 1300A\n\n"+
	  "5 minutovy proud: 1500A\n\n"+
	  "Proud na mezi adheze (skluz): 1548A\n\n"+
	  "Proud na mezi adheze s piskovanim (skluz): 1961A\n\n"+
	  "Autor modelu: Jaroslav Skura, skura@seznam.cz, http://skura.msts.cz/ \n\n"
	 )

	 EngineOperatingProcedures (
	  "Jak se rozjet\n"+
	  "1. Uz máte zvednutý pantograf. (Pokud z nejakého duvodu zvednutý není, stisknete klávesu P pro jeho zvednutí.)\n"+
	  "2. Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
	  "3. Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
	  "(4. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
	  "5. Stisknete D pro zvýsení pozadovaného výkonu.\n"+
	  "6. Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n\n"+
	  "Jak zpomalit\n"+
	  "1. Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
	  "2. Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
	  "Jak pouzít vlakovou brzdu\n"+
	  "1. Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
	  "2. Po dosazení pozadovaného brzd. tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
	  "Jak odbrzdit vlakovou brzdu\n"+
	  "1. Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
	  "2. Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
	  "3. Stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n"+
	  "Jak pouzít lokomotvní brzdu\n"+
	  "1. Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak odbrzdit lokomotivní brzdu\n"+
	  "1. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak pouzít zachrannou brzdu\n"+
	  "1. Stisknete a drzte A pro snízení výkonu az na 0.\n"+
	  "2. Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
	  "Jak zrusit záchrannou brzdu\n"+
	  "1. Pockejte na úplné zastavení vlaku.\n"+
	  "2. Stisknete Z pro odblokování ovládání lokomotivy.\n"+
	  "3. Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
	  "4. Pomalu zvysujte výkon stiskem D .\n\n"+
	  "Jak zmenit smer\n"+
	  "1. Zastavte vlak.\n"+
	  "2. Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
	  "3. Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
	  "4. Pomalu zvysujte vykon stiskem D .\n\n"+
	  "Jak pripojit vagony/lokomotivy\n"+
	  "1. K vagonu musíte prijet pomalu, optimální rychlost je okolo 1 km/h.\n"+
	  "Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
	  "2. Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
	  "3. Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
	  "4. Zavrete okno sestavení vlaku stiskem F9.\n"+
	  "5. Pockejte az odbrzdíte pripojené vozy.\n\n"+
	  "Odpojení vozu nebo lokomotivy\n"+
	  "POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"+
	  "1. Otevrete okno sestavy vlaku F9.\n"+
	  "2. Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
	  "3. Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
	  "4. Pomalu se rozjedte smerem od odpojene casti vlaku.\n"+
	  "(Pozn.: V nekterých prípadech pri rychlejsím odjezdu dojde k opetovnému spojení spráhel. Pokud se toto stane tak soupravu opet rozpojte a velmi pomalu odjízdejte az do vzdálenosti jednoho prazce. Pak jiz muzete zacít zrychlovat.)\n"+
	  "5. Zavrete okno sestavení vlaku stiskem F9.\n\n"
	 ) 
)